IZAR I I1.L2.600.XY
Type: wall lamp. Lampshade: acrylic glass in combination with acrylic glass white (.92), black (.93) or stainless steel (.83). Light body: white painted steel plate.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 20,9 W
Color temperature: 4000 K
Module luminous flux: 2806 lm
Luminaire luminous flux: 2319 lm
A: 600 mm
B: 80 mm
C: 40 mm
Dali 2: Available
Bluetooth control: Available on inquiry
Weight: 1400 g