CHARON PMMA S33.11.CA3.Y
Type: ceiling and wall lamp. Lampshade: acrylic glass PMMA. Light body: white painted steel plate.
Voltage: 230V
IK code: IK06
Socket: E27
Lamps: 1x100W(max 13W LED)
A: 375 mm
B: 330 mm
C: 135 mm
Motion sensor: Available on inquiry
Weight: 1900 g