CHARON PMMA S56.13.CA6.Y
Type: ceiling and wall lamp. Lampshade: acrylic glass PMMA. Light body: white painted steel plate.
Voltage: 230V
IK code: IK06
Socket: E27
Lamps: 3x75W(max 11W LED)
A: 600 mm
B: 560 mm
C: 175 mm
Motion sensor: Available on inquiry
Weight: 4000 g