CHARON IP44 PS29.12.T135.Y
Type: ceiling and wall lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Light body: white painted steel plate.
Voltage: 230V
IK code: IK01
Socket: E27
Lamps: 2x75W(max 11W LED)
A: 360 mm
B: 290 mm
C: 130 mm
Motion sensor: Available on inquiry
Weight: 2900 g