CHARON IP44 PS37.12.T14.Y
Type: ceiling and wall lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Light body: white painted steel plate.
Voltage: 230V
IK code: IK01
Socket: E27
Lamps: 2x75W(max 11W LED)
A: 415 mm
B: 370 mm
C: 125 mm
Motion sensor: Available on inquiry
Weight: 4100 g