CHARON IP44 PS43.13.T15.Y
Type: ceiling and wall lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Light body: white painted steel plate.
Voltage: 230V
IK code: IK01
Socket: E27
Lamps: 3x75W(max 11W LED)
A: 500 mm
B: 430 mm
C: 145 mm
Motion sensor: Available on inquiry
Weight: 5900 g