POLARIS ZT ZT.P2.500.XY
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9003 (.31), RAL 9005 (.61), RAL chrom (.77), chrome (.80), stainless steel (.83) or brass (.84). Pendant: rod.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 37,3 W
Color temperature: 4000 K
Module luminous flux: 6096 lm
Luminaire luminous flux: 5486 lm
A: 500 mm
C: 1000 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Track system: Available on inquiry
Weight: 8100 g