NEMESIS ZL1.11.N250.XY
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9003 (.60), RAL Brass (.74) or chrome (.80). Pendant: steel wire suspension with a transparent cable.
Voltage: 230V
IK code: IK01
Socket: E27
Lamps: 1x75W(max 11W LED)
A: 250 mm
B: 210 mm
C: 2000 mm
Track system: Available on inquiry
Weight: 2700 g