NEMESIS ZL1.11.N350.XY
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9003 (.60), RAL Brass (.74) or chrome (.80). Pendant: steel wire suspension with a transparent cable.
Voltage: 230V
IK code: IK01
Socket: E27
Lamps: 1x100W(max 13W LED)
A: 350 mm
B: 295 mm
C: 2000 mm
Track system: Available on inquiry
Weight: 3800 g