POLARIS ZL PE ZL1.11.400.XY PE
Type: suspension lamp. Lampshade: polyethylene opal PE. Metal parts: painted steel plate RAL 9003 (.31), RAL chrom (.77) or chrome (.80). Pendant: steel wire suspension with a transparent cable.
Voltage: 230V
IK code: IK10
Socket: E27
Lamps: 1x150W(max 19W LED)
A: 400 mm
C: 2000 mm
Track system: Available on inquiry
Sádrokarton: Available on inquiry
Weight: 3200 g