DAPHNE ZL ZL3.L2.D451.31Y
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9003 (.31), RAL chrom (.77). Pendant: wire suspension with white cable.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 32 W
Color temperature: 4000 K
Module luminous flux: 5214 lm
Luminaire luminous flux: 3911 lm
A: 450 mm
B: 200 mm
C: 2000 mm
D: max. 1000 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 6200 g