DAPHNE ZT ZT.13.D550.XY
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Pendant: white painted steel RAL 9003 (.31), chrome (.80), brass (.84), RAL chrom (.77) or RAL Argento dorato (.70) rod suspension.
Voltage: 230V
IK code: IK01
Socket: E27
Lamps: 3x75W(max 11W LED)
A: 550 mm
B: 245 mm
C: 1000 mm
Track system: Available on inquiry
Weight: 8600 g