IZAR B MAX ZL4.IB.L2.1250M.91Y
Type: suspension lamp. Lampshade: acrylic glass. Metal parts: white painted steel plate. Pendant: steel wire suspension with a transparent cable.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 218 W
Color temperature: 4000 K
Module luminous flux: 29136 lm
Luminaire luminous flux: 25120 lm
A: 1250 mm
B: 1250 mm
C: 2000 mm
D: 180 mm
Dali 2: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 49800 g