IZAR B MAX IB.L1.1250M.91Y
Type: ceiling lamp. Lampshade: acrylic glass. Light body: white painted steel plate.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 218 W
Color temperature: 3000 K
Module luminous flux: 27984 lm
Luminaire luminous flux: 24127 lm
A: 1250 mm
C: 180 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 49700 g