IZAR III I3.L1.900.XY
Type: ceiling and wall lamp. Lampshade: acrylic glass, front white (.92) or black (.93). Light body: white painted steel plate.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 30,7 W
Color temperature: 3000 K
Module luminous flux: 4047 lm
Luminaire luminous flux: 3712 lm
A: 900 mm
B: 80 mm
C: 40 mm
Dali 2: Available
Bluetooth control: Available on inquiry
Weight: 2000 g